All parameters were left as default except:

1) Slice spacing was changed from 1.0 to 4.6
using 6.5um pixels/60x mag = 108nm xy pixel size in sample
0.5um piezo step size during acquisition/108nm = 4.6pixels in z

2) Interpolation was changed from unchecked to checked
