Axiohm A794 Minidriver Installation File for Windows 95/98

1.  Unzip the file *.ZIP file to a directory.  Two files constitute 
    the driver:  A794.DRV and OEMSETUP.INF.  You might also need
    UNIDRV.DLL, ICONLIB.DLL, and UNIDRV.HLP; these can be found on 
    the Windows 95/98 CD that came with your PC.
2.  Install this driver by double clicking on 'Add Printer' from the 
    Printers folder.
3.  Advance to the installation wizard screen that shows a list of
    Manufacturers and a list of Printers.  Click the 'Have Disk' button.
4.  Fill in the path to the files you created in Step 1 in the box
    below the caption 'Copy manufacturer's files from:' and hit Enter.
5.  Choose the printer model to suit your needs:
    "Axiohm A794 Partial" - Partial cut, no cash drawer pulse
    "Axiohm A794 Full" - Full cut, no cash drawer pulse
    "Axiohm A794 CD #1 Partial" - Partial cut, cash drawer #1 pulse
    "Axiohm A794 CD #1 Full" - Full cut, cash drawer #1 pulse
    "Axiohm A794 CD #2 Partial" - Partial cut, cash drawer #2 pulse
    "Axiohm A794 CD #2 Full" - Full cut, cash drawer #2 pulse
    "Axiohm A794 COMP Partial" - Partial cut, for use with the Axiohm
        Complete Driver
    "Axiohm A794 COMP Full" - Full cut, for use with the Axiohm Complete
        Driver

Notes:  If you attempt to print a test page, it won't look too good.  If
        you get anything recognizable, take it as a sign that the 
        installation was a success.

        Please configure the printer for A794 Native Emulation when using 
        this driver.

        The A794 driver contains a special "Control" font that has some
        of its characters mapped onto particular commands, as follows:

        'A' - Hex 41 - Dec 65 - Open cash drawer 1
        'B' - Hex 42 - Dec 66 - Open cash drawer 2
        'C' - Hex 43 - Dec 67 - Full knife cut
        'D' - Hex 44 - Dec 68 - Partial knife cut
        'E' - Hex 45 - Dec 69 - Feed past knife or tearbar
        'F' - Hex 46 - Dec 70 - Feed paper 1/2 inch
        'G' - Hex 47 - Dec 71 - Beep
        'H' - Hex 48 - Dec 72 - (Set active and) print logo 1

        These characters work best placed on a separate line.  They
        will occupy the same amount of vertical space as a visible
        character.  This height has been taken into account in the
        feed commands (E and F).

Support

If there are any questions, please contact DriverHelp@Axiohm.COM.
