Axiohm A794 Minidriver Installation File for Windows NT 4.0

1.  Unzip the file *.ZIP file to a directory.  Preserve the directory               
    structure of the zipped files.  Five files constitute the driver:
    A794.DLL, OEMSETUP.INF, I386\RASDD.DL_, I386\RASDDUI.HL_, and 
    I386\RASDDUI.DL_.
2.  Install this driver by double clicking on 'Add Printer' from the 
    Printers folder.
3.  Advance to the installation wizard screen that shows a list of
    Manufacturers and a list of Printers.  Click the 'Have Disk' button.
4.  Fill in the path to the files you created in Step 1 in the box
    below the caption 'Copy manufacturer's files from:' and hit return.
5.  Choose 'Axiohm A794', 'Axiohm A794 CD#1', 'Axiohm A794 CD#2' or 
    'Axiohm A794 COMP'.  The 2nd and 3rd versions generate a pulse to cash 
    drawer 1 or 2, respectively, after each document; and the 4th 
    version does not send the reset (0x1B 0x40) command at the start
    of every document.
6.  All of the above Axiohm A794 minidrivers now come in 'Full' and 
    'Partial' versions, which send a full cut (0x19) or a partial cut 
    (0x1A) respectively, at the end of each document.

Note:  If you attempt to print a test page, it won't look too good.  If
       you get anything recognizable, take it as a sign that the 
       installation was a success.

Exceptions

1.  There is extra space below a line of double high text.
2.  In Windows NT, barcodes must be preceded by a '!' and followed by a '#' 
    to print correctly.  The '!' and '#' will not print as part of the
    barcode data, but are needed by the minidriver to build the barcode
    command that gets sent to the printer.  The '!' and '#' must be in the
    same font and size as the barcode you wish to print.

Support

If there are any questions, please contact Andy.Nye@Axiohm.COM.