ENVI
description = {
  QuickBird data courtesy of DigitalGlobe.}
samples = 1500
lines   = 1500
bands   = 4
header offset = 0
file type = ENVI Standard
data type = 12
interleave = bsq
sensor type = QuickBird
byte order = 0
map info = {UTM, 1.000, 1.000, 476472.000, 4428429.600, 2.4000000000e+000, 2.4000000000e+000, 13, North, WGS-84, units=Meters}
coordinate system string = {PROJCS["UTM_Zone_13N",GEOGCS["GCS_WGS_1984",DATUM["D_WGS_1984",SPHEROID["WGS_1984",6378137.0,298.257223563]],PRIMEM["Greenwich",0.0],UNIT["Degree",0.0174532925199433]],PROJECTION["Transverse_Mercator"],PARAMETER["False_Easting",500000.0],PARAMETER["False_Northing",0.0],PARAMETER["Central_Meridian",-105.0],PARAMETER["Scale_Factor",0.9996],PARAMETER["Latitude_Of_Origin",0.0],UNIT["Meter",1.0]]}
wavelength units = Micrometers
band names = {
 B, G, R, IR}
wavelength = {
 0.485000, 0.560000, 0.660000, 0.830000}
fwhm = {
 0.065000, 0.100000, 0.065000, 0.110000}
