org.cybergarage.upnp.device

## Interface SearchResponseListener

-     public interface SearchResponseListener

  Interface for receiving SSDP search response messages.

  This interface defines the contract for objects that wish to receive SSDP search responses from UPnP devices. It provides a callback mechanism for handling responses to M-SEARCH discovery requests.

  Key features:

  - Device search response callback method
  - Access to raw SSDP packet data
  - Real-time response handling
  - Device discovery result processing

  Implementations of this interface can register with UPnP control points to receive asynchronous responses when devices reply to discovery searches, enabling comprehensive device discovery and network mapping.

- - ### Method Summary

    All Methods Instance Methods Abstract Methods
    Modifier and Type | Method and Description
    --- | ---
    `void` | `deviceSearchResponseReceived(SSDPPacket ssdpPacket)` Called when an SSDP search response is received from a UPnP device.

- - ### Method Detail

    - #### deviceSearchResponseReceived

          void deviceSearchResponseReceived(SSDPPacket ssdpPacket)

      Called when an SSDP search response is received from a UPnP device.
      Parameters:
        `ssdpPacket` - the received SSDP packet containing search response data